****

**GRADE SPECIFICATION**

**PRODUCT NAME:** **Grooved Profile Plank**

SPECIES / GRADE: Oak

PANEL SIZE: NA – sold as sticks

PLANK WIDTH: 5”

PLANK THICKNESS: 5/8”

PANEL THICKNESS NA

MILLING PROFILE(S) Tongue and Groove Planking

PLANK DESIGN: Custom 5/8” Solid

**Species Available and Specifications**

Listed below are specifications for Oak. This is a standard product, can be stained in a variety of colors and textures, with pricing readily available. For other species, we will require 2-3 working days to finalize pricing and final spec.

**Select Oak and Walnut Panel/Stick Characteristics:**

HEARTWOOD/SAPWOOD CONTENT: Mixed

VERTICAL/FLAT SAWN CONTENT: Mixture of vertical and flat sawn grain

KNOT CONTENT: 80% of the board will be clear and free of knots. Knots over 1” will be defected out, knots under 1” will be filled and finished. All surfaces will be sound.


ADDITIONAL CHARACTER None

**Finish Details:** Standard – Water Clear Low VOC Water based urethane 5-sheen top coat.

Optional Class “A” Fire Treatment Available Upon Request

Optional Stain and Texturing Available Upon Request

**Sample Image:**

****

**Detailed Dimensions:**

